The update includes two steps: 

Step 1: K-BUS USB FIRMWARE UPDATE
Step 2: K-BUS USB DRIVER UPDATE IN ETS

NOTE: All old USB devices (to be updated) SHOULD firstly in a version which works with ETS5 (but with problems for updated ETS5),
 or else it will not work for ETS5